: Public <<Functional>> Requirement

Created: | 26.06.2013 10:11:53
Modified: | 25.09.2013 11:14:53
Project: |
Author: | Thomas Batt
Version: | 1.0
Phase: | 1.0
Status: | Proposed
Complexity: | Easy
Difficulty: | Medium
Priority: | Medium
Multiplicity: |
Advanced: |
UUID: | {04584AA6-941C-4357-BC70-F27D0D164F28}
Appears In: |

When the user presses the mode select or enter push button of the motor control system, the preselect speed is automatically set to zero.